**New Product—Tel Tac® Tach Adapter**

The new Tel Tac® Tach Adapter can be used to correct an irregular readout while using a Crane Cams HI-6 or HEI type ignition system, with a digital Tel Tac® brand tachometer.

This lightweight billet unit is completely sealed in soft urethane to protect from vibration and moisture. A convenient #8 size though hole can be used to hard mount under the dash area with a nut/bolt combination or with a zip tie. All leads are color-coded for ease of installation.

­

***Download High Resolution Image Files at www.AutoPressReleases.com***